a Download the attached file and unzip it to current file folder.
b Plug the dash cam to a computer with the short data cable.
c Copy files unzipped file "FW96663A.bin"to dash cam's SD card. (Please make sure the file on the root directory)
d Unplug the dash cam from computer and then the dash cam will be turned off.
e Pull the SD card out from the SD card slot and then insert it back.
f Plug and charge the dash cam to a wall outlet with the phone adaptor. The  dash cam will be turned on, and the RED LED light will  flash. Please kindly wait for about 1 minute.(Please make sure the  dash  cam is  always  being charged during  the update) When finish updating, the dash cam will automatically turn on.